{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["data"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"data","index":0,"n_rows":15,"n_cols":8,"rows_kept":15,"cut":false,"hidden":false,"merged":[[1,2,1,6],[6,2,6,6],[10,2,10,6]]}
[null,null,null,"Level Mam 4Channel ロギング"]
[null,null,"ロギング　間隔"]
[null,null,null,"日","時間","分","秒"]
[null,null,"Log時間間隔：",0,0,1,2,"設定値入力"]
[null,null,"記入例：",0,0,1,2,"例：0日0時間1分2秒間隔で測定値を記録します。"]
[]
[null,null,"ポート番号"]
[null,null,"本体　番号：","1","2","3","4"]
[null,null,"COMポート番号：",6,7,null,null,"設定値入力"]
[null,null,null,null,null,null,null,"使用しない本体は未記入にする。"]
[null,null,"Level 測定値"]
[null,null,"時　間","1","2","3","4"]
[null,null,"2018/06/19/08/07/49",-0.66500000000000004]
[null,null,"2018/06/19/08/08/51",-0.66800000000000004,0.998]
[null,null,"2018/06/19/08/09/53",-0.66500000000000004]